SELECT THE CORRECT STARTUP. I'VE MADE IT SO EASY NOW :)
COPY AND PASTE IT INTO THE ROOT OF YOUR SD FOR RAPHAEL,TOPAZ,BLACKSTONE AND RHODIUM
OR INTO THE INTERNAL STORAGE OF YOUR DIAMOND

STARTUP/DEFAULT.TXT COMMANDS
Overclocking
acpuclock.oc-freq-khz=XXXXXX ( i use 600000 ) 
but it very unstable if you try to get higher than 650000-700000

Physical Keyboard layout
physkeyboard=fuze
physkeyboard=raph
physkeyboard=raph_nordic
physkeyboard=tilt2
physkeyboard=rhod210
physkeyboard=rhod100_de
physkeyboard=rhod100_fr
physkeyboard=rhod100_it
physkeyboard=rhod100_uk
physkeyboard=rhod100_nordic
physkeyboard=rhod400
physkeyboard=rhod500

Button wake up
board-htcraphael-navi.wake=X 
0 =  screen only wakes on power button
1 = wakes on any keypress

Onscreen terminal keyboard
msmvkeyb_toggle= (on/off)
on = displays terminal onscreen keyboard
off = hide terminal onscreen keyboard

LCD density / resolution
lcd.density=XXX
210 = 640x480 VGA devices
240 = 800x480 WVGA devices
